# mmdbresolve(1) Manual Page

## NAME

mmdbresolve - Read IPv4 and IPv6 addresses and print their IP geolocation information.

## SYNOPSIS

mmdbresolve -f <dbfile> [ -f <dbfile> ] …​

## DESCRIPTION

mmdbresolve reads IPv4 and IPv6 addresses on stdin and prints their IP geolocation information on stdout. Each input line must contain exactly one address. Output is in INI format, with a section delimiter named after the query address followed by a set of "key: value" pairs. A comment beginning with "# End" is appended to each section.

At startup an "[init]" section is printed that shows the status of each datbase and of mmdbresolve itself.

## OPTIONS

-f

  Path to a MaxMind Database file. Multiple databases may be specified.

## EXAMPLES

To resolve a single address:

    echo 4.4.4.4 | mmdbresolve -f /usr/share/GeoIP/GeoLite2-City.mmdb

Example output

    [init]
    db.0.path: /usr/share/GeoIP/GeoLite2-City.mmdb
    db.0.status: OK
    mmdbresolve.status: true
    # End init
    [4.4.4.4]
    # GeoLite2-City
    country.iso_code: US
    country.names.en: United States
    location.latitude: 37.751000
    location.longitude: -97.822000
    # End 4.4.4.4

## SEE ALSO

wireshark(1), tshark(1)

## NOTES

mmdbresolve is part of the Wireshark distribution. The latest version of Wireshark can be found at https://www.wireshark.org.

HTML versions of the Wireshark project man pages are available at https://www.wireshark.org/docs/man-pages.

## AUTHORS

Original Author

Gerald Combs <gerald[AT]wireshark.org>